Dominik Kurasbediani

01146313@pw.edu.pl

Continuous Face Detection and Verification During Online Examinations

Abstract

I present a prototype of a system used to continuously detect and verify faces of examinees during online examinations, as well as a method of representation of the results of such verifications, and overall architecture of the system. The system consists of three modules: the client-side face detection, the server-side face verification, and the exam supervisor’s dashboard. Face detection occurs on each client’s computer using *Single Shot Multibox Detection* (SSD). The resulting image is aligned and cropped, then encoded into base-64 format and sent to the verification server via a POST request. Upon receiving such request, the server decodes the base-64 image, feeds it to the *VGG-Face* model to get a vector representation of the face and compares the Euclidean distance between said image and a predefined base image. The results of the last operation are sent to the exam supervisor’s dashboard via a POST request. The exam supervisor’s dashboard’s task is to receive and process such requests and represent the updated data in real time. In addition, the exam supervisor’s dashboard is responsible for configuration of the exam session, as well as generation of the client-side executables to allow easy and seamless process for the students.

Keywords: Real-Time Face Recognition, Client-Server Architecture, Online Examination.

# Abstract in Polish

# Statement about the authorship of the work signed by the student

Table of Contents

[Abstract 1](#_Toc112607490)

[Abstract in Polish 2](#_Toc112607491)

[Statement about the authorship of the work signed by the student 3](#_Toc112607492)

[Motivation 6](#_Toc112607493)

[Existing Procedures 7](#_Toc112607494)

[Proposed Procedure 8](#_Toc112607495)

[Chapter 1. System Architecture 9](#_Toc112607496)

[1.1 Exam Supervisor’s Dashboard 10](#_Toc112607497)

[Frontend 10](#_Toc112607498)

[Backend 13](#_Toc112607499)

[**1.2** **Client-Side Face Detection** 17](#_Toc112607500)

[**ID Form** 17](#_Toc112607501)

[Capture Window 18](#_Toc112607502)

[1.3 Verification Server 20](#_Toc112607503)

[File Handling 20](#_Toc112607504)

[Representation 20](#_Toc112607505)

[Verification 21](#_Toc112607506)

[Chapter 2. Detection Solution Study & Analysis 26](#_Toc112607507)

[Speed 26](#_Toc112607508)

[Accuracy 27](#_Toc112607509)

[ROC 28](#_Toc112607510)

[AUC 28](#_Toc112607511)

[Results 29](#_Toc112607512)

[Resources 30](#_Toc112607513)

[Analysis 30](#_Toc112607514)

[Conclusion 31](#_Toc112607515)

[Chapter 3. VGG-Face 32](#_Toc112607516)

[Network Architecture and Training 32](#_Toc112607517)

[Learning Face Classifier 32](#_Toc112607518)

[Triplet Loss 33](#_Toc112607519)

[Architecture 33](#_Toc112607520)

[Training 34](#_Toc112607521)

[Evaluation and Results 34](#_Toc112607522)

[Chapter 4. Single Shot Multibox Detector (SSD) 36](#_Toc112607523)

[Architecture 36](#_Toc112607524)

[Training 0](#_Toc112607525)

[References 3](#_Toc112607526)

[List of Tables 5](#_Toc112607527)

[List of figures 6](#_Toc112607528)

[List of appendices 7](#_Toc112607529)

[appendices 8](#_Toc112607530)

## Motivation

The current solutions for online examination are variants of the following approach: the students connect to a third party-provided online meeting (e.g., Zoom, Microsoft Teams), turn on their cameras, proceed to complete the exam. This method is flawed in terms of security against academic offenses. The most prevalent one, in my experience as a student, is the abuse of the fact that the exam supervisor has never seen students’ faces before the exam due to it not being required during the semester, as well as the absence of identity verification as a prerequisite to writing the exam. In other words, students may outsource (ask their friends to write the exam for them, pay a professional to do it, or other) and get a passing grade regardless of whether they truly know the material presented during the semester. During the COVID-19 pandemic, when there was no other option other than online education and online exams, the students were incentivized to abuse this system, commit academic offenses, and get a passing grade without opening the course textbook once during the semester. This effectively lowers the overall education level, potentially creating severe errors, which may be lethal in some cases, due to students-turned-professionals being unqualified. One may argue that the proportion of students cheating is marginal at best, however this problem is a hole in a ship that might lead to it sinking.

With an existing state-of-the-art face recognition technology, it is possible to prevent these problems by building and integrating security applications into existing infrastructures of academic institutions.

## Existing Procedures

Normally examinations are held in-person, which prevents students from committing academic offenses under the watchful eyes of the exam supervisors and their assistance. The identity of examinees is established and verified either on entrance to the exam room or during the exam itself: the examinees are asked to present a student identification card that contains the image of their face, first and last name(s), and the student ID number. This information is verified against a list of students registered for this exam, and the images in the identification card is matched with the face of the owner of the card. If these conditions are met, the examinee is cleared to write the exam. Examinees are not allowed to leave the exam room until they have turned in their exam papers, or their identity is verified once again on re-entry.

The described above procedure is put in place with security in mind, to prevent the problem mentioned in the previous section. It has been successful in preventing most cases of identity fraud in the context of examinations. However, currently there is no such procedure being used for online examinations.

## Proposed Procedure

The procedure I use in my application is modeled after the existing in-person exam protocol:

1. Before the start of the exam session, exam supervisors are required to create a list of students allowed to take the exam (first and last names, student numbers, optional base image).
2. The client executables (access point for the students) are generated and distributed to the students.
3. The exam supervisor starts the exam session.
4. The students launch the executables, input their identification data (first and last names, student number)
5. The system verifies their faces throughout the duration of the whole exam.

The described above procedure replicates the in-person procedure except for the last step. Step 6 covers an edge case that is only possible during online examinations: it is not possible to fake one’s identity once it has been verified without leaving the examination room first. However, during online examinations it is possible. By ensuring continuous verification, the application prevents it from happening.

# Chapter 1. System Architecture

Any face recognition pipeline consists of at least four parts: face detection, alignment, face representation, and verification. The system consists of three modules: client-side face detection, server-side face verification, and exam supervisor’s dashboard. The pipeline stages are spread across the three modules to optimally distribute the stress and utilization of computational resources required of each stage. Figure 1 shows the spread of the face recognition pipeline:

Text

Description automatically generated

Figure . Request flow diagram and the spread of the face recognition pipeline. The red rectangles are the stages of the face recognition pipeline.

## Exam Supervisor’s Dashboard

The Dashboard module is responsible for configuration of the session, executing compilation scripts, starting the verification server, and presentation of the verification results. It is a web application that the examination supervisor exclusively will have access to. The module consists of two components: the frontend and the backend.

### Frontend

This component is responsible for the visual representation of the data and allowing the supervisor to utilize all the tools provided efficiently and with ease. The User Interface (UI) is designed to be as minimalistic and intuitive as possible to minimize the training required to become acclimated to the system. It is built with React JS, which is a JavaScript framework. Due to the limitation imposed by the useEffect hook in React JS, it is impossible to use it to automatically refresh the contents of the page whenever there is a change in data. Instead, the contents are manually refreshed with a set frequency. This results in a consistent amount of GET requests to the backend, which is more stable when there is a large number of clients connected to the session.

Timeline

Description automatically generated with medium confidence

Figure . Default UI of the Dashboard

#### Add Student

This button redirects the user to a separate page that contains a form that allows for addition of new students to the database. The required components are the first and last names, and the student identifier. There is also an optional field to add a base image of the student. This base image is uploaded to the backend server and saved locally for the verification purposes. The ‘Cancel’ button redirects the user back to the previous page.




Figure . Add Student Form

When the form is submitted, the contents are sent to the backend via a POST request, where it is processed further. After this step, the student is added to the table on the previous page and to the database.




Figure . Table after a new examinee has been added.

The ‘Delete’ button deletes the given student from the database.

#### Save

The ‘Save’ button saves the current state of the database, serializes it into .json format and the supervisor can download it to their computer.

#### Compile Client Executables

This button starts the compilation of the executables used by clients (examinees) to send the detected faces to the verification server. In case the supervisor does not have the executables, or the configuration of the component, or the component itself, has changed between sessions, it is required to compile new client executables. In the prototype application, this process can take up to approximately 2 hours to finish, and once started the supervisor is asked not to close or refresh the page until the process is finished.

#### Start Session

This button starts the verification server effectively starting the session. Shortly after this step, the supervisor can alert the examinees that the session has begun and ask them to run the distributed executables.

#### Load Save

The ‘Load Save’ is the counterpart to the ‘Save’ button. The supervisor can use this button to upload a previously saved session instead of starting a new one.

### Backend

This component is responsible for all the data management, script execution and operation of the dashboard. It is a REST API built with C# and ASP.NET Core.

#### Database

The module is implemented in a way that omits configuration and maintenance of dedicated databases and instead utilizes an in-memory database built in runtime. This solution reduces the cost of maintenance in the long-term at the cost of building the database every session (which is compensated by the ability of the user to export the session data and load sessions from a .json file). The solution also decreases the amount of time required for the changes to occur due to the lack of the need to send and receive data from a dedicated database. However, it is configured in a way that would not take a significant amount of development time to implement support of a dedicated solution due to utilization of .NET’s Entity Framework.

#### Add Student

Entity Framework and ASP.NET provide a simple and well-documented framework for database operations such as adding, editing, and deleting new entries (POST, PUT and DELETE requests, respectively.) The form sent along with the POST request contains serialized text information regarding the name, surname, and student identifier. The latter is the primary key.

The form may optionally contain an image. If there is an image attached, the server will rename the image to the student identifier the image belongs to postfixed with the extension of the image file and save it locally. The location of the saved image is also recorded in the database to avoid iterating through the directory to delete the image when deleting a student, as well as to supplement session save-load system.

#### Saving

When the server receives a request to save the current session, it serializes the list of students currently in the database into a .json file (name, surname, student identifier, status, last status update and path to the base image). The file is saved locally to the dashboard’s host machine to provide an additional fail-safe to user errors. Then the resulting file is read as an array of bytes. Then the server returns a file with the specified serialized session (Status200OK), the Content-Type of ‘application/octet-stream’, and ‘SaveData.json’ as the name of the file. This file is then sent to the user and is downloaded.

#### Loading

Upon receiving a given POST request to load the session, the server assumes an attached session data file previously generated with the ‘Save’ button. The file is then saved locally on the server’s host machine to allow for diagnostics in case an error occurs. The contents of the file are then deserialized and the list of examinees is added to the existing database.

All the steps are performed inside try-catch blocks to avoid fatal errors due to dealing with file systems. In addition to the assumption stated above, there are null checks at the deserialization step to handle the case where the submitted .json file would contain serialization errors. If the file submitted is empty, the user will receive a Status-400 Bad Request response.

Upon successfully adding all the examinees to the database, the server returns a Status-200 OK response.

#### Compilation Script Execution

To maintain modularity and customizability of the system, the Dashboard relies on Windows Shell or Bash (depending on the host OS) to execute the compilation process. The API itself only starts said scripts. For the prototype, the script first attempts to install all the Python dependencies required by the client. It then attempts to install PyIntsaller – a Python package that allows to bundle the client application and all its dependencies into a single package. The packages that are already present are skipped to avoid redundancies. Once dependency installation has been concluded, the client application is compiled using PyInstaller. The compilation time depends on the technical specifications of the machine is it executed on. However, the first time this process is executed on a machine, it takes a significant amount of time to finish. After the process is finished, PyInstaller does not remove the intermediate files, so further compilation times will take significantly less time. Once the compilation has finished, the resulting files are zipped and sent to the requester.

#### Start Session

The system design expects the verification server and the dashboard to be launched from the same machine. The main reason is session directory preparation. The verification server verifies the incoming faces against their respective base images that are prepared in this step.

Once the dashboard’s server receives a request to start a session, before running any scripts, it starts preparing the directories and file system hierarchy expected by the verification server. First, it deletes the remainder directories from the previous session. Then, it creates a directory for each examinee with the student identifier as the name.

Like the ‘Compilation Script Execution’ section, this procedure uses custom Windows Shell or Bash scripts to allow for customizability and expandability. In the prototype, the script iterates through the base images uploaded through the ‘Add Student’ step, puts them into their respective directory and renames them to ‘base’ followed by the extension of the file. Then the script installs the Python dependencies required by the verification server and starts the server.

## **Client-Side Face Detection**

Once the compilation of client executables is done, the supervisor may distribute them to the examinees. Each examinee gets one executable file for their operating system (.exe for Windows, .app for Mac OS).[[1]](#footnote-1) They will launch this executable right before attempting the exam. The module is responsible for detecting the faces of each examinee. It also crops and aligns the face to the size required and sends the image to the verification server, where it is processed further. The module is written in Python. The Module is divided into two components: the ID form and the capture window.

### **ID Form**

This component is responsible for the presentation of the form the examinees must complete for the detection process to begin. It consists of only one field – the student identifier.

Graphical user interface, application

Description automatically generated

Figure . Client Form

Once completed, the user presses the corresponding buttons, and the identifier entered is saved and is sent with every payload for the verification server to identify the sender. Once the ‘Next’ button is pressed, the form window closes, and the capture window opens starting the face detection process.

### Capture Window

The opened window shows the camera-feed with a rectangle around the detected face (if any) and a number in the top left corner. The number represents the time left before the detection is “unfrozen” (more on this in the backend section)

A picture containing text, person, person, wall

Description automatically generated

Figure . Capture window.

This component is responsible for face detection, alignment, cropping and sending the captured images to the verification server.

#### Face detection

The face detection solution uses ResNet SSD model (Single Shot Multi-Box Detection, more on SSD in Chapter 2) and its pre-trained weights provided by OpenCV community. However, OpenCV’s deep neural network module can load external caffe models, so the solution is expandable, and the model chosen is interchangeable.

Since the model expects a certain sized input, the images taken from the camera are scaled down to that size. Most of the time models require low resolutions (300x300 in case of ResNet SSD), so to maintain modularity and customizability of the system, the images sent to the verification server are scaled back to the original resolution.

The scaled down images are then fed forward to the caffe model. The resulting matrix is then filtered by face features.[[2]](#footnote-2) This produces a set of coordinates that are then scaled up to the original resolution, and the result is a set of coordinates that define the bounding box containing the detected face.

#### Procedures & Error Prevention

To prevent false positives and false negatives, as well as a waste of verification server’s resources, the client will only send the detected face to the verification server if the face has been detected in a set number of consecutive frames. This amount is customizable, and the prototype runs at five consecutive frames.

Since the faces are detected each frame, which can happen more than once per second, sending an image each time requires considerable transmission bandwidth. In addition, the verification server might get overloaded and crash during sessions with a large number of students. To prevent both, after sending an image to the server, the client stops the detection and the process of sending a face for a set time. This time is customizable, and the prototype uses five seconds. During the ‘freeze,’ the image captured in the last frame is cropped to the size of the bounding box so that it only contains the contents of the box. The resulting image is then encoded into a base-64 format and sent to the verification server along with the examinee identifier in the body of a POST request.

## Verification Server

This module is responsible for representation and verification of faces. The start of the verification server signifies the start of the session. Once the session starts, the verification server will receive POST requests containing the cropped images of faces to verify from the clients. Upon receiving such request and handling the resulting files, the server feeds the image to the VGG-Face based CNN to receive a vector representation of the face. It then verifies it against an existing base image that is set during session configuration. The result of the comparison is then sent to the exam supervisor’s dashboard via a POST request, body of which contains the student identifier and the result of verification. The module contains the representation and verification units of the pipeline. It is implemented in Python with the use of Flask framework to manage receiving and sending requests.

### File Handling

Upon receiving a POST request from a client, the server notes the request number and the examinee identifier of the request’s author. First, the server must check whether an examinee that authored the request is registered for the session. It does so by checking the existence of a directory named after the examinee identifier configured via the supervisor’s dashboard prior to the start of the session. While inefficient, it allows for modularity and component flexibility. If it does not, the server ignores the request, otherwise it may proceed further. The server then decodes the received image from base-64. The server then checks whether a base image for the examinee exists. If it does not, it uses the first image received during the session as a base image for that examinee. The server then saves the image locally in the directory of the base image of the examinee. Then, the server then cleans the directory so that up to nine last images and the base image remain. Saving the images to the hard drive is also a measure to handle the case of server crashing, as there are no measures preventing the server from crashing. After that, the representation phase of the pipeline begins.

### Representation

The aim of this phase is to transform the received image to vector form, so that the verification is possible. This done by feeding the image to the VGG-Face based CNN (more on this in Chapter 3) to receive a vector representation of the face. The model itself is state-of-the-art and produces results with 98.95% accuracy when evaluated on LFW (Labeled Faces in the Wild) dataset. (Parkhi, 2015) The model performs better than most state-of-the-art alternatives, including Google’s FaceNet (without alignment 98.87% accuracy) and Facebook’s DeepFace (97.35% accuracy) while requiring less data and using simpler network architecture. (Parkhi, 2015) However, the choice of the model used is customizable and may also be changed to a different one.

Since the image is already aligned and cropped, there is no need for extra face detections and any other pre-processing. Upon receiving the vector representation of an image, the server checks whether the same image already exists, and if it does, the verification result will return ‘false,’ meaning the examinee is cheating. It does so by finding the difference between the vector representation of each image in the directory dedicated to the examinee. If the server did not stop here, it caches the vector representation to memory to optimize the performance. Also, it releases the memory taken by the previous allocation.

The number of allocations is customizable due to the limitations caused by the size of the vector representation. VGG-Face produces a vector of length 2622, so in the prototype the number of caches is set to three per examinee, otherwise there is a risk of exhausting the RAM.

### Verification

Once a vector representation of two images is obtained, it is possible to compare the two. The assumption is that images of the face belonging to the same person will have similar vector representations, within a set margin of error. There are two ways to find how similar the vector representations are considered for this purpose.

#### Euclidean Distance

The Euclidean distance between two vectors may be represented by the following formula:

, (1)

where represents the length of the vector representation of an image.

The verdict on whether the face shown on the first image is the same face shown in the second, may be determined by comparing the obtained in (1) Euclidean Distance to a set threshold value:

In the prototype, Euclidean distance is the verification method of choice, and the threshold is set to 0.55 as recommended by the authors of the model. It is completely customizable, and for stricter results one may want to decrease it.

#### Cosine Distance

Let and be vectors, and be the angle between them.

Chart, line chart

Description automatically generated with medium confidence

Figure . Vectors a and b.

Let vector be equal to . Vectors and create a valid triangle.

Chart

Description automatically generated

Figure . Vectors a, b, and c.

Therefore, the law of cosines states that:

,

where , and are the vector lengths of , and respectively.

Then,

(1)

(2)

(3)

(4)

(5)

(6)

And, from Pythagorean theorem, the length of a vector is:

(7)

Then, by combining (6) and (7), cosine similarity can be defined as:

In this way, similar vectors will produce comparable results. Cosine distance is then defined by:

Like in the case of Euclidean distance, the verdict of whether the face in the first image is the same as the same in the second image is determined by comparing the calculated distance to a set threshold:

#### Verdict

Once a verdict is obtained through comparing Euclidean or Cosine distance to a set threshold, it is packed into the body of a POST request, along with the examinee identifier. The POST request is then sent to the supervisor’s dashboard, where the status of that examinee is updates, along with the last update request time.

# Chapter 2. Detection Solution Study & Analysis

When choosing a solution for face detection, there are three main factors to consider: speed, accuracy and resources required. To choose the optimal detector, a study was conducted. The face detectors considered are:

1. Haar Cascade, offered by OpenCV.
2. Single Shot Multibox Detector (SSD), offered by OpenCV.
3. Histogram of Oriented Gradients (HOG), offered by Dlib.
4. Max-Margin Object Detection (MMOD), offered by Dlib.
5. Multi-task Cascaded Convolutional Network (MTCNN), offered by its own library.

The detectors listed above contain both legacy (Haar Cascade, HOG) and state-of-the-art solutions. The aim of the study is to describe and compare the listed above face detection methods in terms of speed, accuracy and computational resources required. The study is conducted on a 2.6 GHz 6-Core Intel i7 machine with 16 GB 2667 MHz DDR 4 RAM.

## Speed

Each of the above detectors is used to find a face in 6600 consecutive frames containing a single face. The time required to detect the face is recorded. The Activity Monitor is monitored throughout the experiment to find the relative resources taken up by the calculations for each detector (CPU Load & Memory Load).

The results are presented in Table 1 below, Table 6 (in the appendix section), and Figure 9. MMOD is the slowest detector, while Haar Cascade is the fastest on average, with SSD being the close second.

Chart

Description automatically generated with medium confidence

Figure . Chart representing the speed of detection of different face detectors. The values are taken from Table 1.

Table . Detector Speed Comparison

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Detector | HOG | Haar Cascade | MTCNN | SSD | MMOD |
| Avg. per 100 frames (s) | 34.89 | 3.67 | 56.54 | 3.92 | 706.37 |
| Avg. per 1 frame (s) | 0.35 | 0.04 | 0.57 | 0.04 | 7.06 |
| Avg. frames per second: | 2.87 | 27.22 | 1.77 | 25.50 | 0.14 |

## Accuracy

The accuracy of a detector is determined by calculating the Area Under Curve (AUC) of the corresponding Receiver Operating Characteristic Curve (ROC).

### ROC

An ROC curve is a graph showing the performance of a classification model at all classification parameters: True Positive Rate and False Positive Rate.

True Positive Rate (**TPR**) is a synonym for recall and is defined as follows: (“Classification: ROC Curve and AUC - Google Developers”)

where TP is the number of True Positive results, and FN is the number of False Negative results.

False Positive Rate **(FPR**) is defined as follows:

where FP is the number of False Positives, and TN is the number of True Negatives.

An ROC curve plots TPR over FPR at different classification thresholds. Lowering the classification threshold classifies more items as positive. Therefore, it increases both FPR and TPR.

### AUC

Are Under the ROC curve measures the entire two-dimensional area underneath the ROC curve from (0, 0) to (1, 1). The values range from 0 to 1. A detector whose predictions are always wrong across a dataset will have an AUC of 0.0, while a detector whose predictions are always right will have an AUC of 1.0. This metric is desirable for two reasons: it is scale-invariant (measures how well predictions are ranked as opposed to their absolute values), and it is classification-threshold-invariant (measures the quality of the model’s predictions regardless of the classification threshold chosen).

### Results

The accuracy experiments were conducted on the FDDB (Jain, 2010) dataset and the percentages shown are based on AUC values.[[3]](#footnote-3) In descending order of accuracy:

1. MTCNN – ~90% (Wang, 2018)
2. SSD – ~88% (Granger, 2017)
3. MMOD – ~70% (Cheney, 2015)
4. HOG – ~60% (Cheney, 2015)
5. Haar Cascade – ~50% (Pattarapongsin, 2020)

## Resources

The observations are made on the data produced by the Activity Monitor that creates a new output entry every ten seconds. Results are the outputs of the Activity Monitor regarding the average CPU Load and RAM usage over the period of computation, presented in Table 2 and Table 3, respectively.

Table 2. CPU Load Comparison by Detectors

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Detector | HOG | Haar Cascade | MTCNN | SSD | MMOD |
| CPU Load Before (%) | 2.56 | 11.55 | 2.47 | 11.48 | 2.21 |
| CPU Load After (%) | 9.52 | 27.63 | 12.39 | 28.05 | 12.48 |
| Difference (%) | 6.96. | 16.08 | 9.92 | 16.57 | 10.27 |

Table 3. RAM Use Comparison by Detector

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Detector | HOG | Haar Cascade | MTCNN | SSD | MMOD |
| RAM Before (GB) | 7.8 | 6.2 | 10.7 | 6.2 | 10.9 |
| RAM During (GB) | 8.2 | 6.8 | 11.1 | 6.7 | 13.9 |
| Difference (GB) | 0.4 | 0.6 | 0.4 | 0.5 | 3.0 |

## Analysis

While Haar Cascade is one of the fastest methods (avg. 27.22 frames per second), it has the lowest accuracy out of all tested (approx. 50%). Using Haar Cascade may lead to production of inaccurate data even with the error prevention procedures (described in the next section) in place.

HOG is another legacy method that does not compete with the state-of-the-art methods. Not only is the accuracy just approximately 10% better than Haar Cascade but it is also much slower (avg. 2.87 frames per second), despite loading the CPU the least, while using as much RAM as MTCNN.

MTCNN overperforms all tested methods in terms of accuracy (approx. 90%). However, the speed at which it can detect faces (avg. 1.77 frames per second) makes it inapplicable in real-time applications. However, this method is the most efficient in terms of resources used over accuracy.

While MMOD reaches the state-of-the-art status due to its accuracy (approx. 70%), the detection speed is the slowest out of all considered detectors. It is slower than MTCNN by a factor of twelve. It also uses the most resources and would not be feasible in a commercial application – 3 GB of RAM.

SSD is the perfect detector for real time applications due to its fast speed of detection (avg. 25.5 frames per second), high accuracy (approx. 88%) and low resources requirements – lower than Haar Cascade in terms of RAM used and approximately the same CPU Load.

## Conclusion

While all the detectors have their advantages and disadvantages, Single Shot Multibox Detector (SSD) is the perfect detector for real time applications with its low resource use, high speed, and accuracy.

# Chapter 3. VGG-Face

Pre-trained VGG-Face and its derivative (ResNet) models are used during the detection and representation stages of the face recognition pipeline in the prototype. These models are CNN architectures for face identification and verification. Compared to other state-of-the-art models, VGG-Face has a much simpler architecture that achieves state-of-the-art results on several image and video face recognition benchmarks. (Parkhi, 2015) This chapter covers the network architecture, its training, as well as evaluation of the results against existing datasets.

## Network Architecture and Training

This section describes the process of training the CNN, as well as its structure. Due to the unavailability of large quantities of training data to the public, the training process was omitted in the implementation of the prototype and instead a model with pretrained weights (provided by the OpenCV community) is used. The data set used to train the model contains 2622 identities with up to one thousand images per identity. (Parkhi, 2015)

### Learning Face Classifier

Let denote the deep architecture considered. Initially, they are bootstrapped by structuring the problem of recognizing individuals as a N-ways classification problem. This improves the training speed, as well as makes the training simpler. (Parkhi, 2015)

Let denote each training image. The CNN associates each training image one score vector per identity with the use of final fully connected layer containing linear predictors . The score vectors are compared to the ground-truth class identity . It is accomplished by computing the softmax log-loss:

where e­c denotes the one-hot vector of class c.

After learning, the classifier layer can be removed, and the score vectors can be used for face identity verification. This corresponds to the pre-trained weights in the prototype. The identity verification can be performed by finding the Euclidean distance as described in Chapter 1. However, the scores can be further improved by adjusting them for verification in Euclidean space using *triplet loss* training scheme.

### Triplet Loss

The goal of this training is to improve the learning scores by comparing face descriptors in Euclidean space. The output pretrained is -normalized and projected to a dimensional space using

where .

Note that unlike in the linear predictor from the previous section, is not equal to the number of class identities but is the size of the descriptor embedding (the authors of VGG-Face set . Also, the projection is trained to minimize *triplet loss*:

where is a fixed scalar called *learning margin*, and is a collection of *learning triplets.*

The learning bias is also canceled in the differences in the above equation. From the learning triplet , is the *anchor* face image, and are positive and negative examples of anchor’s identity, respectively.

### Architecture

The detailed architecture of the CNN is given in Table 7. It comprises of eleven blocks, a linear operator followed by one or more non-linearities (ReLU or max pooling). (“Comparative Study of Human Age Estimation Based on Hand-Crafted and ...”) The first eight blocks are exclusively linear convolutions, whereas the remaining three are Fully Connected (FC) – linear convolutions where the size of the filters matches the size of the input data. The first two FC layers output a 4096-dimensional vector, while the last FC layer has dimensions. The resulting vector then passes through a softmax layer to compute the class posterior probabilities.

The input is a face image of size with the average face image subtracted. The average face image is computer from the from the training set.

### Training

According to *Parkhi et al. (2015), l*earning the N-way face classifier follows the steps described by *Krizhevsky, Sutskever and Hinton (2012)* with modifications described by *Simonyan and Zisserman (2014)*. The goal of training is to find parameters of the CNN to minimize the average prediction log-loss after the softmax layer. The optimization happens through stochastic gradient descent (SGD) in batches of 64 samples and momentum coefficient of 0.9, and the model is regularized using dropout and weight decay. The model was trained using three decreasing learning rates. (*Parkhi et al., 2015*)

During training, the network is fed with random pixel patches cropped from the images from the training set, with crops changing every time an image was sampled. The color channel augmentations mentioned in *Krizhevsky, Sutskever and Hinton (2012)* and *Simonyan and Zisserman (2014)* were not applied, whereas the images were flipped horizontally with 50% probability. (*Parkhi et al., 2015*)

For learning using triplet loss, the CNN, except for the last Fully Connected layer, is frozen. The FC layer is then learnt for ten epochs using SGD with a fixed learning rate of 0.25. An epoch contains all positive pairs , where is the anchor image and is its paired positive example. To ensure balanced learning, each pair is extended to a triplet , where is selected at random, such that it violates triplet loss margin. This avoids training with examples that are too hard. (*Parkhi et al., 2015*)

## Evaluation and Results

While the training was done on an original dataset assembled by *Parkhi et al. (2015),* to allow for comparison to other state-of-the-art models, evaluation is performed on existing benchmark datasets – LFW and YTF.

Table 4 and Table 5 below compare the accuracy results of the VGG-Face model to other state-of-the-art models using the LFW and YFD benchmark datasets, respectively. The accuracy is calculated the same way it is described in Chapter 2.

Table . LFW unrestricted settings.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No | Method | Images | Networks | Accuracy |
| 1 | Fisher Vector Faces | - | - | 93.10 |
| 2 | DeepFace | 4M | 3 | 97.35 |
| 3 | Fusion | 500M | 5 | 98.37 |
| 4 | DeepID-2,3 |  | 200 | 99.47 |
| 5 | FaceNet | 200M | 1 | 98.87 |
| 6 | FaceNet + Alignment | 200M | 1 | 99.63 |
| 7 | VGG-Face | 2.6M | 1 | 98.95 |

Table . YFD unrestricted settings. K indicates the number of faces used to represent each video.[[4]](#footnote-4)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No | Method | Images | Networks |  | Accuracy |
| 1 | Video Fisher Vector Faces | - | - |  | 83.8 |
| 2 | DeepFace | 4M | 1 |  | 91.4 |
| 3 | DeepID-2,2+,3 | - | 200 |  | 93.2 |
| 4 | FaceNet + Alignment | 200M | 1 |  | 95.1 |
| 5 | VGG-Face (K=100) | 2.6M | 1 |  | 91.6 |
| 6 | VGG-Face (K=100) + Embedding learning | 2.6 | 1 |  | 97.3 |

# Chapter 4. Single Shot Multibox Detector (SSD)

SSD is a method for detecting objects in images using a single neural network. Compared to methods that require object proposals, it is easy to train because it does not rely on proposal generation or subsequent pixel (or feature) resampling and encapsulates all computation in a single network. *(W. Liu et al., 2016)* Hence, integration into face recognition pipelines does not entail a cost that would normally appear when switching detectors. SSD is the first deep learning-based method that does not resample pixels or features for bounding box hypothesis and is as accurate as the methods that do while maintaining higher speeds of detection.

This section covers the detection method in detail. Some experiments regarding comparison to other state-of-the-art solutions have already been conducted and analyzed in Chapter 2.

## Architecture

The method relies on feed-forward CNN to produce a fixed-size collection of bounding boxes and scores, which used to determine the presence of instances of a set object class on the boxes. The method uses ResNet (a network based on VGG-16 up to layer *conv5\_3,* described in Chapter 3), further referred to as *base network*. *W. Liu et al. (2016)* add auxiliary structure that produce detections with multi-scale feature maps, convolutions predictors, and default boxes and aspect ratios.

To support the multi-scale feature maps feature, *W. Liu et al. (2016)* add convolutional feature layers to the end of the base network, which progressively decrease in size allowing predictions of detections with multiple scales. The detection prediction model is unique to each feature layer. Each extra feature layer may use a set of convolutional filters (denoted in the figure below) to produce those detection predictions.

Diagram, engineering drawing

Description automatically generated

Figure . ResNet SSD network structure.

Let denote the size of a feature layer and denote the number of channels in that feature layer. A potential prediction’s parameters are predicted with a filter of size , which produces a score for a category (or an offset relative to the default box coordinates).

For multiple feature maps at the top of the network, a default bounding box is associated for each cell. The default boxes are positioned in a way that ensures that the position of each box relative to its corresponding cell is fixed. At each cell, the offsets relative to the default box shapes in the cell arepredicted, as well as the scores per class that signify the presence of an instance of that class in each of those boxes. For an feature map, for each default box out of at a given location, class scores are computed along with four offsets relative to the original default box shape. These yield outputs with filters. By applying default boxes to several feature maps at different resolutions, the model efficiently approximates the space of possible output box shapes.

## Training

While SSD is comparatively easier to train than other object detectors, the problem of the availability of annotated datasets of faces described in the previous chapter persists, which forced the use of a pre-trained model in the prototype. Nevertheless, it is important to note that the training process of SSD differs from other detectors that use region proposals. Namely, the ground truth information must be assigned to specific outputs in the fixed set of detector outputs. A prerequisite to training the model is choosing a set of default boxes and scales for detection. It is also necessary to choose hard negative mining and data augmentation strategies.

Each ground truth box, selected from a set of default boxes of varying locations, scaling and aspect ratios, is matched to the default box with the best Jaccard overlap. This is done to determine which default boxes correspond to ground truth during training. Then, default boxes that have a Jaccard overlap with any ground truth higher than a set threshold, are matched. This avoids making the network to pick only one default box with maximum overlap, allowing the network to pick multiple overlapping boxes, which simplifies the learning problem.

The training objective of SSD is the extended version of MultiBox. (*W. Liu et al., 2016)* Let be the result of matching the -th default box to -th ground truth in category . The objective loss function is defined as follows:

,

where N is the number of matched default boxes, is localization loss (Smooth L1 loss between predicted box and ground truth box ), is confidence loss, is classes confidence, and is the weight term, which is set to 1 by cross validation. The offsets for the bounding box center are regressed for its width and height.

To improve and smoothen the semantic segmentation results, *W. Liu et al. (2016)* use feature maps from both upper and lower layers of the network. This helps capture more details from the input. Increasing the number of feature maps does not cause a huge increase of computational overhead. Moreover, the default boxes are designed in a way to allow specific feature maps learn to respond to certain scales of objects. The scale of default boxes for each feature map is computed using the formula:

where is the number of feature maps used for prediction, is the scale of the lowest layer, and is the scale of the highest layer. It is also assumed that all layers are spaces regularly. Let the set of different aspect ratios is applied to the default boxes be denoted as . The w

idth and the height of the default boxes is computed using the following formulas, respectively:

Also, in the case of , and additional default box with is added, resulting in six default boxes per feature map location. Each default box’s center is set to , where is the size of the -th square feature map, and .

The combination predictions for all default boxes with different scales and aspect ratios achieves a diverse set of predictions, which covers a vast amount of input object sizes and shapes. This, however, leads to most default boxes being negative matches. In order to balance the positive and negative examples during training, the negative examples are sorted by descending confidence loss for each default box and the first ones are picked in a fashion that preserves the ratio of 3:1 of negatives to positives. *W. Liu et al. (2016)* suggest that tis is the leads to faster optimization and a more stable training.

References

Liu, W., Anguelov, D., Erhan, D., Szegedy, C., Reed, S., Fu, C. Y., & Berg, A. C. (2016, October). Ssd: Single shot multibox detector. In European conference on computer vision (pp. 21-37). Springer, Cham.

Zhang, K., Zhang, Z., Li, Z., & Qiao, Y. (2016). Joint face detection and alignment using multitask cascaded convolutional networks. IEEE signal processing letters, 23(10), 1499-1503.

Ren, S., He, K., Girshick, R., & Sun, J. (2015). Faster r-cnn: Towards real-time object detection with region proposal networks. Advances in neural information processing systems, 28.

Gao, X., Xu, J., Luo, C., Zhou, J., Huang, P., & Deng, J. (2022). Detection of Lower Body for AGV Based on SSD Algorithm with ResNet. Sensors, 22(5), 2008.

Serengil, S. I., & Ozpinar, A. (2020, October). Lightface: A hybrid deep face recognition framework. In 2020 innovations in intelligent systems and applications conference (ASYU) (pp. 1-5). IEEE.

Simonyan, K., & Zisserman, A. (2014). Very deep convolutional networks for large-scale image recognition. arXiv preprint arXiv:1409.1556.

Owusu, E., Abdulai, J. D., & Zhan, Y. (2019). Face detection based on multilayer feed‐forward neural network and haar features. Software: Practice and Experience, 49(1), 120-129.

Cheney, J., Klein, B., Jain, A. K., & Klare, B. F. (2015, May). Unconstrained face detection: State of the art baseline and challenges. In 2015 International Conference on Biometrics (ICB) (pp. 229-236). IEEE.

Ma, Mei, and Jianji Wang. "Multi-view face detection and landmark localization based on MTCNN." In 2018 Chinese Automation Congress (CAC), pp. 4200-4205. IEEE, 2018.

Granger, E., Kiran, M., & Blais-Morin, L. A. (2017, November). A comparison of CNN-based face and head detectors for real-time video surveillance applications. In 2017 Seventh International Conference on Image Processing Theory, Tools and Applications (IPTA) (pp. 1-7). IEEE.

Pattarapongsin, P., Neupane, B., Vorawan, J., Sutthikulsombat, H., & Horanont, T. (2020, July). Real-time drowsiness and distraction detection using computer vision and deep learning. In Proceedings of the 11th International Conference on Advances in Information Technology (pp. 1-6).

Jain, V., & Learned-Miller, E. (2010). Fddb: A benchmark for face detection in unconstrained settings (Vol. 2, No. 6). UMass Amherst technical report.

Parkhi, O. M., Vedaldi, A., & Zisserman, A. (2015). Deep Face Recognition. British Machine Vision Conference.

Krizhevsky, A., Sutskever, I., & Hinton, G. E. (2012). Imagenet classification with deep convolutional neural networks. Advances in neural information processing systems, 25.

Simonyan, K., & Zisserman, A. (2014). Very deep convolutional networks for large-scale image recognition. arXiv preprint arXiv:1409.1556.

List of Tables

[Table 1. Detector Speed Comparison 27](#_Toc112607294)

[Table 2. CPU Load Comparison by Detectors 30](#_Toc112607295)

[Table 3. RAM Use Comparison by Detector 30](#_Toc112607296)

[Table 4. LFW unrestricted settings. 35](#_Toc112607297)

[Table 5. YFD unrestricted settings. K indicates the number of faces used to represent each video. 35](#_Toc112607298)

[Table 6. Time It Took to Detect a Face In 100 Frames for Each Detector in The Study 8](#_Toc112607299)

[Table 7. Network Configuration 11](#_Toc112607300)

List of figures

[Figure 1. Request flow diagram and the spread of the face recognition pipeline. The red rectangles are the stages of the face recognition pipeline. 9](#_Toc112606845)

[Figure 2. Default UI of the Dashboard 10](#_Toc112606846)

[Figure 3. Add Student Form 11](#_Toc112606847)

[Figure 4. Table after a new examinee has been added. 11](#_Toc112606848)

[Figure 5. Client Form 17](#_Toc112606849)

[Figure 6. Capture window. 18](#_Toc112606850)

[Figure 7. Vectors a and b. 23](#_Toc112606851)

[Figure 8. Vectors a, b, and c. 23](#_Toc112606852)

[Figure 9. Chart representing the speed of detection of different face detectors. 27](#_Toc112606853)

[Figure 10. ResNet SSD network structure. 36](#_Toc112606854)

List of appendices

appendices

Table . Time It Took to Detect a Face In 100 Frames for Each Detector in The Study

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Frames | HOG (34.89 s) | Haar Cascade (3.67 s) | MTCNN (56.54 s) | SSD (3.92 s) | MMOD (706.37 s) |
| 0 | 1.91E-06 | 3.10E-06 | 1.19E-06 | 9.54E-07 | 9.54E-07 |
| 100 | 36.23554897 | 2.892754078 | 52.70409131 | 3.675975084 | 714.192678 |
| 200 | 38.19530511 | 3.647857904 | 57.03780794 | 3.940686941 | 702.5152059 |
| 300 | 39.1812408 | 3.586294889 | 56.46708608 | 3.945479155 | 700.4858158 |
| 400 | 39.52439189 | 3.651924849 | 56.37909412 | 4.010371923 | 714.3655293 |
| 500 | 39.90351486 | 3.553075314 | 55.89740419 | 3.955664158 | 726.1441998 |
| 600 | 38.74442697 | 3.743636131 | 56.03834772 | 4.008642197 | 717.1490119 |
| 700 | 36.33512497 | 3.65500474 | 56.02677226 | 3.957942724 | 718.219789 |
| 800 | 36.13481593 | 3.626913071 | 56.51862001 | 3.983809948 | 713.509789 |
| 900 | 35.70137191 | 3.620682955 | 56.81792307 | 3.991145372 | 713.1944649 |
| 1000 | 34.73823833 | 3.790052176 | 57.09005785 | 3.95042491 | 714.4203029 |
| 1100 | 34.61590981 | 3.94590497 | 56.62220502 | 3.909925938 | 712.8579521 |
| 1200 | 34.57207179 | 4.153652906 | 56.41286898 | 3.943305969 | 713.2627251 |
| 1300 | 35.18846607 | 3.911190033 | 56.37266803 | 3.955844879 | 715.407809 |
| 1400 | 35.89384604 | 3.903182983 | 57.96661687 | 3.945614815 | 713.1372221 |
| 1500 | 34.77288485 | 3.768427134 | 56.94543505 | 3.962347984 | 714.8470218 |
| 1600 | 35.16177893 | 3.756734133 | 56.12602091 | 3.933098078 | 714.520968 |
| 1700 | 36.26053715 | 3.859287024 | 56.91828895 | 3.993356705 | 714.2139311 |
| 1800 | 34.80420804 | 3.635421991 | 56.9134059 | 3.941020012 | 722.8619452 |
| 1900 | 34.76336527 | 3.672314167 | 56.83629584 | 4.894211054 | 776.919234 |
| 2000 | 34.73393321 | 3.660866022 | 56.36047101 | 4.656308174 | 716.854419 |
| 2100 | 34.82744288 | 4.037606955 | 57.07335114 | 4.396603107 | 713.9079881 |
| 2200 | 34.90236497 | 3.958940029 | 57.12043285 | 3.994015932 | 714.0851352 |
| 2300 | 34.8298192 | 3.943880081 | 57.02983022 | 3.901252985 | 714.5670102 |
| 2400 | 34.78930902 | 3.836150885 | 56.69914913 | 3.934653044 | 716.274045 |
| 2500 | 34.81329298 | 3.83989501 | 56.71609712 | 3.947287083 | 716.9648211 |
| 2600 | 34.89078975 | 3.60651803 | 56.802001 | 3.969969034 | 715.0454102 |
| 2700 | 35.40051413 | 3.874823809 | 57.01909995 | 3.938131094 | 714.5149717 |
| 2800 | 34.92322326 | 3.715693951 | 57.05367613 | 3.946982861 | 716.5775499 |
| 2900 | 35.02890015 | 3.854228973 | 57.70291305 | 3.915117741 | 714.1904569 |
| 3000 | 34.89464712 | 3.760348797 | 56.80151296 | 3.96803093 | 715.6364722 |
| 3100 | 34.92685199 | 3.763174057 | 57.54318213 | 3.922150135 | 716.953058 |
| 3200 | 34.91502595 | 3.861320972 | 58.38510585 | 3.938748837 | 714.8684709 |
| 3300 | 34.86225367 | 3.693748951 | 57.2086637 | 3.930501938 | 718.7691603 |
| 3400 | 34.87888098 | 3.656505823 | 56.935462 | 3.978216887 | 715.604208 |
| 3500 | 34.86684799 | 3.625830889 | 56.95947814 | 3.966948032 | 719.419198 |
| 3600 | 34.88854241 | 3.786928892 | 57.3007431 | 3.874152899 | 722.7068 |
| 3700 | 34.86988211 | 3.728536129 | 58.29726315 | 3.999593973 | 716.939121 |
| 3800 | 35.60413408 | 3.853372812 | 63.3768971 | 3.971475124 | 721.0257149 |
| 3900 | 34.85610509 | 3.770243168 | 64.4227891 | 3.950376272 | 754.906004 |
| 4000 | 34.73978376 | 3.616067171 | 63.72983575 | 3.9523561 | 756.9659011 |
| 4100 | 34.72175217 | 3.62292695 | 63.14247298 | 3.965316057 | 712.736068 |
| 4200 | 34.75443697 | 3.969269991 | 60.87343502 | 3.932665825 | 713.4003789 |
| 4300 | 34.6889441 | 3.708190918 | 56.85196495 | 3.969374895 | 713.6921852 |
| 4400 | 34.63854909 | 3.766145945 | 56.5027101 | 4.000520945 | 713.2438259 |
| 4500 | 34.71834493 | 4.037469149 | 56.80987072 | 3.946408033 | 713.7064109 |
| 4600 | 34.61712503 | 3.885704041 | 55.02467823 | 4.004537821 | 714.096406 |
| 4700 | 34.90109587 | 3.82043314 | 56.53544235 | 3.733859777 | 712.7653639 |
| 4800 | 34.93319106 | 3.691066027 | 56.81591392 | 3.700518847 | 713.1198988 |
| 4900 | 34.95742893 | 3.65775609 | 59.53966475 | 3.975763083 | 716.5449371 |
| 5000 | 34.86180305 | 3.567481041 | 56.77645206 | 3.996060848 | 714.6663461 |
| 5100 | 34.822685 | 3.633549213 | 57.48884678 | 3.981528044 | 713.2522249 |
| 5200 | 34.72906613 | 3.679870844 | 57.1327889 | 3.94652009 | 713.5582352 |
| 5300 | 34.95375896 | 3.695036888 | 56.53270698 | 3.974726915 | 712.8458319 |
| 5400 | 35.0191102 | 3.691630125 | 56.1580832 | 3.938524246 | 713.5904951 |
| 5500 | 34.988446 | 3.690860987 | 56.40633416 | 4.167500019 | 715.3053761 |
| 5600 | 34.94446492 | 3.760370016 | 56.73422885 | 3.941513062 | 714.889977 |
| 5700 | 34.99821973 | 3.625473976 | 56.89035892 | 4.070861816 | 712.391938 |
| 5800 | 34.8733511 | 3.603440046 | 57.03578591 | 3.926305056 | 715.3215871 |
| 5900 | 34.83911896 | 3.669696093 | 56.52842903 | 3.976537704 | 716.0530481 |
| 6000 | 34.96892524 | 3.651811123 | 58.10961103 | 3.976406097 | 713.9290781 |
| 6100 | 34.81871414 | 3.716593266 | 58.40186977 | 3.925348997 | 714.1170731 |
| 6200 | 34.84648705 | 3.619926929 | 57.31867075 | 3.955195189 | 713.8299489 |
| 6300 | 34.82126904 | 3.642750978 | 57.5792222 | 3.954037189 | 713.993417 |
| 6400 | 35.00901389 | 3.68410778 | 57.96823192 | 3.961057186 | 714.4916289 |
| 6500 | 41.56679916 | 3.683916092 | 58.05325794 | 3.897565842 | 716.917402 |
| 6600 | 35.2322619 | 3.524402857 | 58.05020332 | 3.948808908 | 715.40253 |

Table . Network Configuration

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Layer | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 |
| Type | Input | conv | relu | Conv | Relu | Mpool | Conv | Relu | Conv |
| Name | - | Conv1\_1 | Relu1\_1 | Conv1\_2 | Relu1\_2 | Pool1 | Conv2\_1 | Relu2\_1 | Conv2\_2 |
| Support | - | 3 | 1 | 3 | 1 | 2 | 3 | 1 | 3 |
| Filt dim | - | 3 | - | 64 | - | - | 64 | - | 128 |
| Num filts | - | 64 | - | 64 | - | - | 128 | - | 128 |
| Stride | - | 1 | 1 | 1 | 1 | 2 | 1 | 1 | 1 |
| Pad | - | 1 | 0 | 1 | 0 | 0 | 1 | 0 | 1 |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Layer | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16 | 17 |
| Type | Relu | Mpool | Conv | Relu | Conv | Relu | Conv | Relu | Mpool |
| Name | Relu2\_2 | Pool2 | Conv3\_1 | Relu3\_1 | Conv3\_2 | Relu3\_2 | Conv3\_3 | Relu3\_3 | Pool3 |
| Support | 1 | 2 | 3 | 1 | 3 | 1 | 3 | 1 | 2 |
| Filt dim | - | - | 128 | - | 256 | - | 256 | - | - |
| Num filts | - | - | 256 | - | 256 | - | 256 | - | - |
| Stride | 1 | 2 | 1 | 1 | 1 | 1 | 1 | 1 | 2 |
| Pad | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 0 |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Layer | 18 | 19 | 20 | 21 | 22 | 23 | 24 | 25 | 26 |
| Type | Conv | Relu | Conv | Relu | Conv | Relu | Mpool | Conv | Relu |
| Name | Conv4\_1 | Relu4\_1 | Conv4\_2 | Relu4\_2 | Conv4\_3 | Relu4\_3 | Pool4 | Conv5\_1 | Relu5\_1 |
| Support | 3 | 1 | 3 | 1 | 3 | 1 | 2 | 3 | 1 |
| Filt dim | 256 | - | 512 | - | 512 | - | - | 512 | - |
| Num filts | 512 | - | 512 | - | 256 | - | - | 512 | - |
| Stride | 1 | 1 | 1 | 1 | 1 | 1 | 2 | 1 | 1 |
| Pad | 1 | 0 | 1 | 0 | 1 | 0 | 0 | 1 | 0 |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Layer | 27 | 28 | 29 | 30 | 31 | 32 | 33 | 34 | 35 |
| Type | Conv | Relu | Conv | Relu | Mpool | Conv | Relu | Conv | Relu |
| Name | Conv5\_2 | Relu5\_2 | Conv5\_3 | Relu5\_3 | Pool5 | Fc6 | Relu6 | Fc7 | Relu7 |
| Support | 3 | 1 | 3 | 1 | 2 | 7 | 1 | 1 | 1 |
| Filt dim | 512 | - | 512 | - | - | 512 | - | 4096 | - |
| Num filts | 512 | - | 512 | - | - | 4096 | - | 4096 | - |
| Stride | 1 | 1 | 1 | 1 | 2 | 1 | 1 | 1 | 1 |
| Pad | 1 | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 |

|  |  |  |
| --- | --- | --- |
| Layer | 36 | 37 |
| Type | Conv | Softmx |
| Name | Fc8 | Prob |
| Support | 1 | 1 |
| Filt dim | 4096 | - |
| Num filts | 1024 | - |
| Stride | 1 | 1 |
| Pad | 0 | 0 |

1. The prototype is limited to only producing executables for the host machine’s OS. It can be expanded using Docker or utilizing a different bundler. [↑](#footnote-ref-1)
2. The naming for these features will also differ depending on the model used, so filtering depends on the model used. [↑](#footnote-ref-2)
3. The accuracies are taken from their respective references [↑](#footnote-ref-3)
4. All the data is taken from *Parkhi et al. (2015).* [↑](#footnote-ref-4)